|  |  |
| --- | --- |
| **A** | 건축도면 표기약자 |
| **AB** | anchor bolt, 앵커볼트 |
| **ABS** | asbestos, 석면 |
| **AC** | air conditioner |
| **AD** | aluminium door, automatic door, air duct |
| **AW** | Aluminium window |
| **ACST** | acoustic |
| **AL** | aluminium |
| **AP** | access pannel |
| **ASPH** | asphalt, 아스팔트 |
| **ATC** | acoustic texture coating |
| **B** | bath, 욕실 |
| **B, BM** | beam |
| **BD** | board |
| **BLDG** | building |
| **BLK** | block |
| **BLT** | bolt |
| **B.M** | bench mark, bench marking, 기준점 |
| **B/M** | bill of material |
| **B.P** | base plate |
| **BRK** | brick, 벽돌 |
| **B.S** | both side |
| **BSMT** | basement |
| **C** | column. 기둥 |
| **CAT.** | catalog |
| **CH.** | chimney |
| **CL.** | closet |
| **CLG.** | ceiling |
| **CLKG.** | coulking |
| **CLR.** | clearance, clear |
| **CMU.** | concrete masonry unit |
| **COL.** | column |
| **CONC.** | concrete |
| **CORR.** | corridor |
| **C. PLAS** | concrete plaster |
| **CONTR. JT** | construction joint |
| **C TO C, C.T.C** | center to center. 중심간 |
| **D** | depth |
| **D** | 일반철근, 일반철근의 직경(mm) : 구조도면 중 배근도에서 |
| **DET** | detail. 상세도 |
| **DIA** | diameter. 지름 |
| **DIM** | dimension, 치수 |
| **DJ** | dummy joint |
| **DN** | down |
| **DP** | damp proofing |
| **DR** | door, drain |
| **DWG** | drawing |
| **E** | 전기설비도면 표기약자, 전기설비중 소방설비는 EF |
| **EA** | each |
| **ECB** | exposed concrete block |
| **ED** | electrical duct |
| **EJ, E.JT, EXT.JT** | expansion joint |
| **EL , ELEV** | elevation |
| **ELEC** | electrical |
| **ELEV** | elevator |
| **ENT** | entrance. 현관 |
| **EQUIP** | equipment |
| **ERP** | epoxy resin paint |
| **EXP** | expansion, exposed(노출) |
| **EXT** | exterior. 외부 |
| **F** | fixed. 고정, 창호도에서는 고정창 |
| **F** | footing. 기초 |
| **FD** | floor drain |
| **F. DR** | fire door. 방화문 |
| **FL** | floor, floor level |
| **FDN** | foundation |
| **FB** | foundation beam |
| **FG** | footing girder. 지중보- 기초간 연결보 |
| **FIN** | finished |
| **FR** | frame |
| **FTG** | footing |
| **G** | girder |
| **GAL** | gallon |
| **GALV** | galvanized |
| **GB** | grade beam |
| **GCB** | glazed concrete block |
| **GCT** | glazed concrete tile |
| **GL** | ground level. 지반고 |
| **GYP** | gypsum. 석고 |
| **H** | height, H-beam |
| **H.B.B / HBB** | HORIZONTAL BOTTOM BUILDING |
| **H.C.B / HCB** | HIGH CEILING BUILDING |
| **HD** | highbar diameter, 하이바, 고강도철근의 직경(mm) : 구조도면중 배근도에서 |
| **HDR** | High Damping Rubber 면진구조에 사용되는 고감쇠고무 |
| **HDW** | hardware |
| **HRB** | high roof beam |
| **HT** | heught |
| **INS** | insulation |
| **INT** | interior |
| **JT** | joint |
| **K, KIT** | kitchen |
| **KP** | kick plate |
| **LAV** | lavatory. 실험실 |
| **L.E.B / LEB** | LIGHTWEIGHT PRE-ENGINEERED BUILD SYSTEM |
| **LDK** | living + dining + kitchen |
| **LIV** | living room |
| **LTR** | lighting |
| **LVR** | louvers |
| **M** | 기계설비도면 표기약자, 기계설비중 소방설비는 MF |
| **MAR** | marble |
| **M.B / MB** | MODULAR BUILDING |
| **MECH** | mechanical. 기계(설비) |
| **MEZZ** | mezzanine |
| **M.F.B / MFB** | MEZZANINE FLOOR BUILDING |
| **M.G.B / MGB** | MULTI-GABLE BUILDING |
| **MH** | menhole |
| **MO** | masonry opening |
| **M.S.B / MSB** | MONO SLOPE BUILDING |
| **NS** | non-slip |
| **OP** | oil paint |
| **OPEN, OPNG** | opening. 개구부 |
| **P** | parking |
| **PC** | precast |
| **PCB** | precast cement base |
| **PD** | pipe duct, plastic door |
| **P.E.B / PEB** | PRE-ENGINEERED METAL BUILDING SYSTEM |
| **PLAS** | plaster |
| **PL** | plate |
| **PS** | pipe shaft |
| **PT** | precast terrazzo |
| **PTB** | precast terrazzo base |
| **PW** | plastic window |
| **PWD** | ply wood |
| **RC** | reinforced concrete |
| **RD** | roof drain |
| **RF** | roof. 지붕 |
| **RM** | room |
| **RWP** | rain water pipe |
| **S** | structure, structural 구조도면 표기약자 : 도면표지 또는 도면분류기호에서 |
| **S, SC** | scale. 축척 : 건축도면에서 |
| **S** | slab. 슬라브 : 구조도면에서 |
| **S.C.S** | STANDARD CLEAR SPAN BUILDING |
| **SD** | steel door |
| **SECT** | section |
| **SHT** | sheet |
| **SPEC** | specification |
| **SS, SST** | stainless steel |
| **SSD** | stainless steel door |
| **SS** | steel shutter |
| **ST, STL** | steel |
| **ST** | stair |
| **STR** | structural |
| **SYM** | symbol |
| **T** | toilet. 화장실 : 실명의 약자로 사용시 |
| **TEMP** | temperature |
| **TER** | terrazzo |
| **THK** | thickness |
| **TOC** | top of concrete |
| **TYP** | typical |
| **UT** | utility |
| **VAR** | vaiable |
| **VCB** | vinyl cover base |
| **VENT** | ventilator, ventilation |
| **VERT** | vertical |
| **VP** | vinyl paint, vanish paint |
| **W** | wall : 구조도면에서 |
| **W** | width. 폭 |
| **WC** | water closet. 화장실 |
| **WD** | wood door |
| **WF** | wall footing. 줄기초 : 구조도면에서 |
| **WW** | wood window. 목재창 : 창호도에서 |